QUALITY SPECIFICATIONS

THE BUILDING

Foundation
Made with reinforced concrete footings.
Structure
Formed by pillars, slabs, and stairs of reinforced concrete.
Facade and Roof
The facade is finished with a combination of single-layer plaster in various colors and made waterproof with exterior paint.
Exterior finishing with SATE insulation layer.
Separations between apartments are acoustically insulated.
Covering with various types of flooring on the roof, with thermal insulation and waterproofing through a membrane, below the floor level.
Sustainable construction, with energy savings and improvement of comfort in the top-floor apartments.
Common Areas
On the stairs to the apartments, ceramic tiles / natural stone treads and concrete railings finished with monocapa.
Energy Classification
The apartments have energy class A.









APARTMENT

Masonry
Exterior walls with double masonry and intermediate thermo-acoustic insulation in accordance with CTE. Interior partition walls with double 7 cm hollow bricks, coated with cement mortar, and partition walls between apartments with double partition walls and acoustic insulation.
Tiling
Combination of high-quality domestic ceramic tiles from floor to ceiling in bathrooms, combined with areas finished with paint.

Floors
1st quality domestic porcelain floors in the apartments, with white porcelain skirting boards.
Laminate floors with wood finish of choice.
For the terraces on the ground floor and the private roof terrace, high-quality domestic anti-slip ceramic tiles are used, with additional thermal insulation on the roof.
Continuous coating
Continuous plastering with white plaster on vertical walls, with PVC profiles. False ceilings of plasterboard in corridors and bathrooms, with removable panels in one bathroom.
Painting
Plastic paint with smooth finish throughout the house. Walls in broken gray and ceilings in white.
Interior Carpentry
Reinforced entrance door with security locking points, lacquered white or wood color on the inside and finished with PVC panel on the outside in a color of choice.
Interior doors, height 2.03 m, with smooth panels, finished in white, with handles and fittings.
Exterior Carpentry
Lacquered aluminum throughout the house, with sliding windows, except in bathrooms with tilt and turn or hinged window. Balcony doors with sliding window.
Windows and balconies with double glazing with sun regulation or similar, according to project calculations.
Plumbing
Consists of an external connection to the water meters, connections to homes, and internal pipes in the home with hot and cold water.
Shut-off valves per home, in bathrooms, kitchen, and toilets, with bithermal water outlets for washing machine and dishwasher.
Hot water pipes, insulated to limit heat loss. PVC drainage pipes, made in accordance with standards.

Domestic hot water (DHW) is individually produced by aerothermal equipment and electric resistance support in the laundry room/kitchen.
Toilets
Toilets from a Spanish top brand, both in the common bathroom and in the main bedroom bathroom.
Shower trays in all bathrooms finished with resin or similar material.
Mixer taps in showers, sinks, and sinks.
Stainless steel sink.

Electricity
Installation with medium level of electrification, with protections in the switchboard against overcurrent and leakage current, with all metal elements of the house and building connected to the grounding in the foundations.
Installation of video intercom with color screen in all homes. Mechanisms from top brands.

Ventilation
To comply with the CTE requirements for air ventilation in homes, they are equipped with the following ventilation systems:
• For kitchens: forced smoke ventilation with an integrated hood with individual duct to the roof.

Air Conditioning/Heating
Pre-installation of hot/cold air conditioning, supply via ducts and return via grilles in dropped ceiling (heat pump not included).
Kitchen
Kitchen and front in compact PVC, equipped with lower and upper cabinets, drawer fronts and doors in a combination of white laminate and wood laminate.
