

Comfort
· Double exterior walls with thermal brick and 6 cm thick XPS thermal insulation system.
· Minimalist anodized aluminum frames by Sosoares with thermal break.
· Heat pumps for hot sanitary water.
· Apartments with energy rating A/A+.
· Centralized electric blinds in the bedrooms.
· High-security entrance doors for apartments by Dierre.
· Switch Otis Gen2 elevator powered by solar panels.
· Daikin air conditioning embedded in ducts throughout the apartment.
· Electric underfloor heating throughout the apartment with remote control.
· Electric garage door.
· Smart home system by Hager with remote control for the entire apartment.
· Tempered laminated glass balcony railings.
· Garage spaces equipped with charging points for electric vehicles.
· Private storage in the basement.
· Heated swimming pool water via heat pump.
· Outdoor area for physical exercise.
Structural Elements
· Foundations with footings and reinforced concrete retaining walls with water-repellent additives.
· Partition walls between apartments with double layers of brick and intermediate air cavity with thermal and acoustic insulation in rock wool.
· All concrete slabs with thermal and acoustic insulation.
· Roof slab in concrete with 8 cm thermal insulation, coated with asphalt mesh.
Interiors
· High-density ceramic flooring by Marazzi, in 120x60 panels, smoothed with rectified joints, reference Carácter Mix Gris Natural Floor Tile.
· False ceilings made of plasterboard panels painted with antifungal plastic paint and embedded lighting by Arkoslight or equivalent.
· Open-plan kitchen integrated with the living room, featuring a Silestone/Dekton countertop.
· Lacquered kitchen cabinets lined with natural wood panels.
· Siemens/Bosch appliances and Bora induction cooktop.
· Shower walls finished with New Terracotta ceramic tiles.
· Fantini faucets, Duravit sanitary ware, and Foursteel electric towel rails.
· Shower cabins with tempered glass doors.
· Bathroom furniture by Querkus or equivalent, with Silestone countertops and sinks.
· Closets by Sangiacomo or equivalent.

